# 1 "/opt/topspin1.3/exp/stan/nmr/lists/pp/kum_mfa-cosy-relay"
;kumar
;pau_cosy-relay

# 1 "/opt/topspin1.3/exp/stan/nmr/lists/pp/Avance.incl" 1
;Avance.incl
;
;avance-version (03/02/17)


















































































































;$Id: Avance1.incl,v 1.10 2003/02/25 14:46:08 ber Exp $
# 4 "/opt/topspin1.3/exp/stan/nmr/lists/pp/kum_mfa-cosy-relay" 2

# 1 "/opt/topspin1.3/exp/stan/nmr/lists/pp/Grad.incl" 1
;Grad.incl  -  include file for Gradient Spectroscopy
;
;avance-version (02/05/31)
;
;$CLASS=HighRes Incl
;$COMMENT=



















define list<gradient> EA=<EA>



;$Id: Grad1.incl,v 1.7.10.1 2005/11/10 13:18:56 ber Exp $
# 5 "/opt/topspin1.3/exp/stan/nmr/lists/pp/kum_mfa-cosy-relay" 2


"d0=3u"
"d13=4u"

1 ze
2 d1
3 50u
  p1 ph1
  d0
  d13 setnmr2|0 setnmr0|34|32|33
  p16:gp1
  d16
  p1 ph2
  d13
  p16:gp1
  d16
  goscnp ph31
  d13 wr #1 
  p16:gp2
  d16
  p1 ph11
  d13
  p16:gp2*-1
  d16 
  goscnp ph31
  d13 wr #2 
  p16:gp3*-1
  d16
  p1 ph11
  d13
  p16:gp3
  d16 
  goscnp ph31
  d13 wr #3 
  p16:gp4
  d16
  p1 ph11
  d13
  p16:gp4*-1
  d16 setnmr2^0 setnmr0^34^32^33
  gosc ph31
  d1 wr #4 
  lo to 3 times 2
  30u if #1
  30u if #2
  30u if #3
  30u if #4
  30u id0
  lo to 3 times td1
  
exit

ph1=0 2 
ph2=0
ph11=1  
ph31=0 2


;pl1 : f1 channel - power level for pulse (default)
;p0 : f1 channel -  20 to 90 degree high power pulse
;p1 : f1 channel -  90 degree high power pulse
;p16: homospoil/gradient pulse
;d0 : incremented delay (2D)                         [3 usec]
;d1 : relaxation delay; 1-5 * T1
;d13: short delay                                    [4 usec]
;d16: delay for homospoil/gradient recovery
;in0: 1/(1 * SW) = 2 * DW
;nd0: 1
;NS: 1 * n
;DS: 16
;td1: number of experiments
;FnMODE: QF

;use gradient ratio:	gp 1 : gp 2
;			  10 :   10

;for z-only gradients:
;gpz1: 10%
;gpz2: 10%

;use gradient files:   
;gpnam1: SINE.100
;gpnam2: SINE.100



;$Id: cosygpqf,v 1.3 2002/06/12 09:04:27 ber Exp $
